Spring Make Ready 2021

**PO Box 686 Holderness, NH 03245**

**(603) 968 8600**

***Please read through and fill out ALL the information below. Incomplete forms will not be accepted.***

Name \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Billing Address\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Summer Address/Location by Water (if applicable) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Primary Phone: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_(Other)\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Email\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

MAKE/MODEL\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_BOW #\_\_\_\_\_\_\_\_\_\_\_I would like my boat completed on **(Date)** \_\_\_\_\_**/\_\_\_\_\_/­­­\_\_\_\_\_\_\_**

**Boat Location:** Stored with NH Mobile Marine\_\_\_\_ I will drop off ***7 days prior to request date***\_\_\_\_ Pick up (fee may apply) \_\_\_\_

**When boat is complete:** Deliver by water\_\_\_\_ Deliver boat on trailer\_\_\_\_ I will pick up my boat on trailer \_\_\_\_

**Select ONE:** 🞏 No trailer 🞏 I will pick up trailer 🞏 Deliver Trailer (fee may apply) 🞏Trailer Storage

**Please choose ONE service level *or* leave blank for required service only:***.*

1. 🞏 Factory Recommended Service including Basic Make Ready

(*Highly recommended yearly for trouble free boating*)

Complete Manufacturer’s suggested tune up.

1. 🞏Tune as Needed including Basic Make Ready

The Technician will determine whether the run condition is

satisfactory or if a tune up is required.

**Options 3 and 4 are REQUIRED**

1. 🗷Basic Make Ready – includes but not limited to:

Charge battery, clean battery terminals, check all fluid levels, all vessel systems and accessories. Check safety equipment. Change water separator filters and fuel filters (Stern drives: inspect bellows, clean flame arrestor). Run engine, check engine systems. Launch and water test vessel.

1. 🗷Unforeseen Repairs

**\*\*Please call if unforeseen repairs exceed $\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (please fill in amount)**

e.g. Blowers, bilge pumps, horns, navigational lights, snaps, covers etc.

**Cleaning**

🞏 **No Clean** 🞏 **Quick Clean**  🞏 **Full Clean-Interior/Exterior** 🞏 **Bottom Wash**

(Vacuum, wipe down, clean glass) (Detail clean. Exterior also washed. Does not include bottom wash.)

**Additional Services**

🞏 **Fill Gas Tank**

🞏**Stern Drive Service** (Recommended every two years)

Stern drive is removed; u-joints, gimble bearing, shafts and splines are inspected and greased. Reinstall with new gasket mounting hardware.

🞏**Health Check**

For engines equipped with onboard computer systems. A computerized diagnostic analysis of engine systems and running conditions.

🞏**Trailer Service**

Check overall condition, tire pressure, lights, grease.

**Signature** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ **Date** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Additional Notes/Requests:**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\*\*I hereby authorize the above work to be done with necessary materials. You and your employees may operate the unit on any waterways or elsewhere for purpose of testing, inspection or delivery at my risk. An expressed mechanics lien is acknowledged on the above unit to secure the number of repairs there. It is also understood that you will not be held responsible for loss or damage to the unit (or articles left in or with the unit) in case of fire, theft, accident, inclement weather conditions or any other cause beyond your control.